
Lab - Troubleshoot Connectivity Issues

# Topology



# Addressing Table

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Device | Interface | IP Address | Subnet Mask | Default Gateway |
| R1 | G0/0/0/1 | 192.168.1.1 | 255.255.255.0 | N/A |
| R1 | G0/0/0 | 10.1.1.1 | 255.255.255.252 | N/A |
| ISP | G0/0/0 | 10.1.1.2 | 255.255.255.252 | N/A |
| ISP | Lo0 | 209.165.200.226 | 255.255.255.255 | N/A |
| S1 | VLAN 1 | 192.168.1.2 | 255.255.255.0 | 192.168.1.1 |
| PC-A | NIC | 192.168.1.10 | 255.255.255.0 | 192.168.1.1 |

# Objectives

Part 1: Identify the Problem

Part 2: Implement Network Changes

Part 3: Verify Full Functionality

Part 4: Document Findings and Configuration Changes

# Background / Scenario

In this lab, the company that you work for is experiencing problems with their Local Area Network (LAN). You have been asked to troubleshoot and resolve the network issues. In Part 1, you will connect to devices on the LAN and use troubleshooting tools to identify the network issues, establish a theory of probable cause, and test that theory. In Part 2, you will establish a plan of action to resolve and implement a solution. In Part 3, you will verify full functionality has been restored. Part 4 provides space for you to document your troubleshooting findings along with the configuration changes that you made to the LAN devices.

**Note**: The routers used with CCNA hands-on labs are Cisco 4221 with Cisco IOS XE Release 16.9.4 (universalk9 image). The switches used in the labs are Cisco Catalyst 2960s with Cisco IOS Release 15.2(2) (lanbasek9 image). Other routers, switches, and Cisco IOS versions can be used. Depending on the model and Cisco IOS version, the commands available and the output produced might vary from what is shown in the labs. Refer to the Router Interface Summary Table at the end of the lab for the correct interface identifiers.

# Required Resources

* 2 Routers (Cisco 4221 with Cisco IOS XE Release 16.9.4 universal image or comparable)
* 1 Switch (Cisco 2960 with Cisco IOS Release 15.2(2) lanbasek9 image or comparable)
* 1 PC (Windows with a terminal emulation program, such as Tera Term)
* Console cables to configure the Cisco IOS devices via the console ports
* Ethernet cables as shown in the topology\

# Troubleshooting Configuration

The following settings must be configured on the devices shown in the topology. Paste the configurations onto the specified devices prior to starting the lab.

S1:

no ip domain-lookup

hostname S1

ip domain-name ccna-lab.com

username admin01 privilege 15 secret cisco12345

interface FastEthernet0/1

shutdown

interface FastEthernet0/2

shutdown

interface FastEthernet0/3

shutdown

interface FastEthernet0/4

shutdown

interface FastEthernet0/5

speed 10

duplex half

interface Vlan1

ip address 192.168.1.2 255.255.255.0

ip default-gateway 192.168.1.0

banner motd $ Authorized Users Only! $

line vty 0 4

login local

transport input ssh

line vty 5 15

login local

transport input ssh

crypto key generate rsa general-keys modulus 1024

end

R1:

hostname R1

no ip domain lookup

ip domain name ccna-lab.com

username admin01 privilege 15 secret cisco12345

interface GigabitEthernet0/0/1

ip address 192.168.1.1 255.255.255.0

no negotiation auto

speed 100

no shutdown

interface GigabitEthernet0/0/0

ip address 10.1.1.1 255.255.255.252

no shutdown

banner motd $ Authorized Users Only! $

line vty 0 4

login local

transport input ssh

crypto key generate rsa general-keys modulus 1024

end

ISP:

hostname ISP

no ip domain lookup

interface GigabitEthernet0/0/0

ip address 10.1.1.2 255.255.255.252

no shut

interface Lo0

ip address 209.165.200.226 255.255.255.255

ip route 0.0.0.0 0.0.0.0 10.1.1.1

end

## Identify the Problem.

The only available information about the network problem is that the users are experiencing slow response times and that they are not able to reach an external device on the internet at IP address 209.165.200.226. To determine probable cause(s) for these network issues, you will need to utilize network commands and tools on the LAN equipment shown in the topology.

**Note**: The user name **admin01** with a password of **cisco12345** will be required to log into the network equipment.

### Troubleshoot the network.

Use the tools available to you to troubleshoot the network, keeping in mind that the requirement is to restore connectivity to the external server and the eliminate slow response times.

**Note**: While using SSH to connect to network devices, issue the **terminal monitor** privileged exec command to enable log output to the SSH console.

### Document the probable causes.

List the probable causes for the network problems that employees are experiencing.

Type your answer here.

## Implement Network Changes

You have communicated the problems that you discovered in Part 1 to your supervisor. She has approved these changes and has requested that you implement them.

## Verify Full Functionality

Verify that full functionality has been restored. PC-A, S1, and R1 should be able to reach the external server, and ping replies from PC-A to the external server should exhibit no significant variation in response times.

## Document Findings and Configuration Changes

Use the space provided below to document the issues found during your troubleshooting and the configurations changes made to resolve those issues.

Type your answers here.

# Reflection Question

This lab had you troubleshoot all devices before making any changes. Is there another way to apply the troubleshooting methodology?

Type your answers here.

# Router Interface Summary Table

| Router Model | Ethernet Interface #1 | Ethernet Interface #2 | Serial Interface #1 | Serial Interface #2 |
| --- | --- | --- | --- | --- |
| 1800 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 1900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2801 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 2811 | Fast Ethernet 0/0 (F0/0) | Fast Ethernet 0/1 (F0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 2900 | Gigabit Ethernet 0/0 (G0/0) | Gigabit Ethernet 0/1 (G0/1) | Serial 0/0/0 (S0/0/0) | Serial 0/0/1 (S0/0/1) |
| 4221 | Gigabit Ethernet 0/0/0 (G0/0/0) | Gigabit Ethernet 0/0/1 (G0/0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |
| 4300 | Gigabit Ethernet 0/0/0 (G0/0/0) | Gigabit Ethernet 0/0/1 (G0/0/1) | Serial 0/1/0 (S0/1/0) | Serial 0/1/1 (S0/1/1) |

**Note**: To find out how the router is configured, look at the interfaces to identify the type of router and how many interfaces the router has. There is no way to effectively list all the combinations of configurations for each router class. This table includes identifiers for the possible combinations of Ethernet and Serial interfaces in the device. The table does not include any other type of interface, even though a specific router may contain one. An example of this might be an ISDN BRI interface. The string in parenthesis is the legal abbreviation that can be used in Cisco IOS commands to represent the interface.

End of document