{"text_format":"1","workbook":"xlsx","n_sheets":2,"sheets":["kmitočtová odezva","L-R tracking"],"not_rendered":{"charts":2,"images":0,"macros":1,"external_links":0,"defined_names":1,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"kmitočtová odezva","index":0,"n_rows":30,"n_cols":9,"rows_kept":30,"cut":false,"hidden":false,"merged":[[1,1,2,1],[1,2,2,2],[1,3,2,3],[1,4,2,4],[1,8,2,8],[1,6,2,6],[1,7,2,7],[1,5,2,5]]}
[]
[null,"kmitočet [Hz]","rel. kmit. odezva ucha umělé hlavy v difúzním poli [dB]","kmit.odezva sluchátek HATS [dB(SPL)]","kmit.odezva sluchátek HATS v ERP [dB(SPL)]","rel.kmit. odezva sluchátek HATS [dB]","rel.kmit. odezva sluchátek HATS v ERP [dB]","kmit.odezva sluchátek umělé ucho [dB(SPL)]","rel.kmit.odezva sluchátek (umělé ucho) [dB]"]
[]
[null,50,0,null,{"$f":"D4-C4","v":0},{"$f":"D4-$D$17","v":0},{"$f":"E4-$D$17","v":0},null,{"$f":"H4-$H$17","v":0}]
[null,63,0,null,{"$f":"D5-C5","v":0},{"$f":"D5-$D$17","v":0},{"$f":"E5-$D$17","v":0},null,0]
[null,80,0,null,0,0,0,null,0]
[null,100,0,null,0,0,0,null,0]
[null,125,0,null,0,0,0,null,0]
[null,160,0,null,0,0,0,null,0]
[null,200,0.27,null,-0.27,0,-0.27,null,0]
[null,250,0.33,null,-0.33,0,-0.33,null,0]
[null,315,0.44,null,-0.44,0,-0.44,null,0]
[null,400,0.63,null,-0.63,0,-0.63,null,0]
[null,500,0.84,null,-0.84,0,-0.84,null,0]
[null,630,0.93,null,-0.93,0,-0.93,null,0]
[null,800,1.0900000000000001,null,-1.0900000000000001,0,-1.0900000000000001,null,0]
[null,1000,1.52,null,-1.52,0,-1.52,null,0]
[null,1250,2.19,null,-2.19,0,-2.19,null,0]
[null,1600,2.4900000000000002,null,-2.4900000000000002,0,-2.4900000000000002,null,0]
[null,2000,3.16,null,-3.16,0,-3.16,null,0]
[null,2500,4.45,null,-4.45,0,-4.45,null,0]
[null,3150,6.52,null,-6.52,0,-6.52,null,0]
[null,4000,9.1,null,-9.1,0,-9.1,null,0]
[null,5000,9.19,null,-9.19,0,-9.19,null,0]
[null,6300,6.31,null,-6.31,0,-6.31,null,0]
[null,8000,1.81,null,-1.81,0,-1.81,null,0]
[null,10000,0.54,null,-0.54,0,-0.54,null,0]
[null,12500,-4.32,null,4.32,0,4.32,null,0]
[null,16000,-9.67,null,9.67,0,9.67,null,0]
[null,20000,-12,null,12,0,12,null,0]

{"sheet":"L-R tracking","index":1,"n_rows":37,"n_cols":5,"rows_kept":37,"cut":false,"hidden":false,"merged":[[1,1,1,4]]}
[]
[null,"Rozdíl přenosové funkce levého a pravého kanálu sluchátek"]
[]
[null,"f","L","R","L-R"]
[null,"[Hz]","[dB]","[dB]","[dB]"]
[]
[null,20,null,null,{"$f":"C7-D7","v":0}]
[null,25,null,null,{"$f":"C8-D8","v":0}]
[null,31.5,null,null,0]
[null,40,null,null,0]
[null,50,null,null,0]
[null,63,null,null,0]
[null,80,null,null,0]
[null,100,null,null,0]
[null,125,null,null,0]
[null,160,null,null,0]
[null,200,null,null,0]
[null,250,null,null,0]
[null,315,null,null,0]
[null,400,null,null,0]
[null,500,null,null,0]
[null,630,null,null,0]
[null,800,null,null,0]
[null,1000,null,null,0]
[null,1250,null,null,0]
[null,1600,null,null,0]
[null,2000,null,null,0]
[null,2500,null,null,0]
[null,3150,null,null,0]
[null,4000,null,null,0]
[null,5000,null,null,0]
[null,6300,null,null,0]
[null,8000,null,null,0]
[null,10000,null,null,0]
[null,12500,null,null,0]
[null,16000,null,null,0]
[null,20000,null,null,0]